Manual d'usuari
La traducció d'aquesta pàgina encara no està acabada. Fins que ho sigui, algunes part correspondrà a la versió anglesa.

# Carregador d'Arrencada

El Carregador d'Arrencada del Haiku us pot ajudar si teniu experiència amb problemes del maquinari o voleu triar una opció per instal·lar el Haiku, si en teniu més d'una (potser una instal·lació amb un CD o amb un llapis USB).
També pot ser útil després que hagueu instal·lat un component de programari que no us permet arrencar el sistema, i per això la voleu eliminar. L'opció Inhabilita les extensions de l'usuari indicada a continuació, permet arrencar el Haiku sense els components instal·lats per l'usuari, per exemple, un connector.

Per accedir a les opcions del Carregador, heu de mantenir premuda la tecla Majúscules abans de començar el procés de càrrega del Haiku. Si hi ha un carregador instal·lat, podeu començar mantenint premuda la tecla Majúscules abans de lleçar el procés de càrrega del Haiku. Si l'únic sistema operatiu del sistema és el Haiku, podeu començar mantenint premuda la tecla i veure al mateix temps els missatges de l'arrencada de la BIOS.

## Boot Loader Options

Un cop aquí se us ofereixen quatre menús:

Selecció del volum d'arrencada |  | Trieu la instal·lació del Haiku que voleu executar.
Select safe mode options |  | En cas de problemes amb el maquinari, hi ha algunes opcions que podeu provar. A la part inferior de la pantalla podeu veure una breu explicació de la opció seleccionada.

Safe mode
Puts the system into safe mode. This can be enabled independently from the other options.

Disable user add-ons
Prevents all user installed add-ons from being loaded. Only the add-ons in the system directory will be used. See Troubleshooting below.

Disable IDE DMA
Disables IDE DMA, increasing IDE compatibility at the expense of performance.

Ignore memory beyond 4 GiB
Ignores all memory beyond the 4 GiB address limit, overriding the setting in the kernel settings file.

Use fail-safe video mode
The system will use VESA mode and won't try to use any video graphics drivers.

Disable IO-APIC
Disables using the IO APIC for interrupt routing, forcing the use of the legacy PIC instead.

Disable local APIC
Disables using the local APIC, also disables SMP.

Disable SMP
Disables all but one CPU core.

Don't call the BIOS
Stops the system from calling BIOS functions.

Disable APM
Disables Advanced Power Management hardware support, overriding the APM setting in the kernel settings file.

Disable ACPI
Disables Advanced Configuration and Power Interface hardware support, overriding the ACPI setting in the kernel settings file.

Blacklist entries
Allows to select system files that shall be ignored. Useful e.g. to disable drivers temporarily. See Troubleshooting below.

Select debug options |  | Trobareu algunes opcions que us poden ajudar a depurar i obtenir més detalls sobre l'error. De nou, a la part inferior de la pantalla podeu veure una breu explicació de l'opció seleccionada.

Enable serial debug output
Turns on forwarding the syslog output to the serial interface (default: 115200, 8N1).

Enable on screen debug output
Display debug output on screen while the system is booting, instead of the normal boot logo.

Disable on screen paging
Disables paging when on screen debug output is enabled.

Enable debug syslog
Enables a special in-memory syslog buffer for this session that the boot loader will be able to access after rebooting.

Display current boot loader log
Displays the debug info the boot loader has logged (press Q to exit the log)

Add advanced debug option
Allows advanced debugging options to be entered directly.

|  | If "Enable debug syslog" is activated, a warm reboot after a crash shows these additional options:
|  | Save syslog from previous session during boot Saves the syslog from the previous Haiku session to /var/log/previous_syslog when booting. Display syslog from previous session Displays the syslog from the previous Haiku session Save syslog from previous session Saves the syslog from the previous Haiku session to disk. Currently only FAT32 volumes are supported.
Selecció del mode de vídeo segur |  | Si heu activat l'opció Usa el mode de vídeo segur, podeu indicar la resolució i la profunditat de color.

## Troubleshooting

If Haiku refuses to boot on your hardware from the get-go, try out setting different options under Select safe mode options. Consider filing a bug report in any case.

On the other hand, if Haiku only suddenly acts up after you have installed some software, especially hardware drivers, you have several options to get Haiku bootable again to make things right by uninstalling the offending package again:

- Activating Safe mode will prevent most servers, daemons and the UserBootScript from being started.

- Activating Disable user add-ons will prevent using any add-ons (drivers, translators, etc.) you have installed in the user hierarchy under your Home folder.

- If the offending driver, add-on etc. is installed in the system hierarchy, things get a bit more complicated, because that area is read-only. Here, the Blacklist entries comes into play. With it, you can navigate through the whole system hierarchy and disable the component that's messing things up for you by checking an entry with the SPACE or RETURN key. ESC returns you up one level to the parent directory.

  Online, there's the article How to Permanently Blacklist a Package File showing how to make that setting stick.

## Booting Haiku

Després d'activar qualsevol opció, tornareu al menú principal i el sistema continuarà amb el procés d'arrencada, que mostrarà aquesta pantalla:

Si tot funciona correctament, apareixeran successivament uns símbols.
Els símbols corresponent aproximadament a aquestes etapes del procés d'arrencada:

Atom |  | S'estàn iniciant els mòduls.
Disc + lupa |  | S'estàn creant el guió rootfs (/) i muntant el fitxers devfs (/dev).
Targeta d'ampliació |  | S'està iniciant el gestor de dispositius.
Disc d'arrencada |  | S'està muntant el disc d'arrencada.
Xip |  | S'estàn carregant els mòduls de la CPU.
Carpeta |  | S'han iniciat tots els subsistemes.
Coet |  | El guió d'arrencada està engegant el sistema.