User guide
The translation of this page isn't yet complete. Until it is, unfinished parts use the English original.

## Завантажувач

Deskbar: |  | Не входить, звичайно запускається з меню Інструменти Встановлювача
Розміщення: |  | /boot/system/apps/BootManager(Завантажувач)
Настройки: |  | жодних Попередній запис MBR по замовчуванню зберігається в ~/config/settings/bootman/

Якщо Ви не додавали розділ з Haiku до наявного завантажувача такого ,наприклад ,як GRUB, Завантажувач встановить маленьке загрузочне меню до MBR, Яке може виглядати десь отак:

Завантажувач не є протестованим до кінця, тому накладаються обмеження, про які Ви не повинні забувати: меню може бути встановлене тільки на перший жорсткий диск, на ньому має бути принаймні 2KiB вільного місця після основного загрузочного запису (MBR).

Завантажувач буде супроводжувати Вас у процесі встановлення загрузочного меню.

## Вибір диску призначення

The BootManager starts off with a list of all available drives from which you choose the destination. If there's already a boot menu on that drive, the Uninstall button becomes active, leading you through the simple procedure to restore a formerly backed-up MBR, thereby removing the boot menu again.
Otherwise, choose Install to continue.

## Backing up the Master Boot Record (MBR)

In case anything goes wrong or you want to remove the boot menu again, the Master Boot Record (MBR) is now saved. This is obviously a very important step, make sure you don't accidentally overwrite some other MBR-backup maybe from some earlier experimentation, for example!

Just select a destination for the backup file "`MBR`" or leave the default path. After clicking Next you'll get a confirmation if the backup was successful.

## Configuring the boot menu

Next you're presented with a list of all partitions on the destination drive. By setting checkmarks you decide what entries will appear in the boot menu, the text boxes allow you to rename an entry.

After that, you pick from the pop-up menu which partition will be booted from by default and set a timeout with the slider below. Here, "Immediately" will skip the boot menu entirely, "Never" will just stop at the boot menu. You can override the timeout setting by holding ALT while booting.

## Writing the boot menu

Before the boot menu is written to the MBR, you'll get a summary of your configuration and then one last chance to abort the operation. Don't worry though, as long as you keep the MBR backup safe, you can easily revert the changes. Should things get thoroughly messed up, you can always boot from a Haiku install CD or USB stick and write back the MBR backup with BootManager.